SSP(1)

NAME
ssp - The Single Step Profiler

SYNOPSIS

ssp [-cdelstv] low_pc high_pc command...

ssp -h | -V

OPTIONS

     -c, --console-trace  trace every EIP value to the console. *Lots* slower.
     -d, --disable        disable single-stepping by default; use
                          OutputDebugString ("ssp on") to enable stepping
     -e, --enable         enable single-stepping by default; use
                          OutputDebugString ("ssp off") to disable stepping
     -h, --help           output usage information and exit
     -l, --dll            enable dll profiling.  A chart of relative DLL usage
                          is produced after the run.
     -s, --sub-threads    trace sub-threads too.  Dangerous if you have
                          race conditions.
     -t, --trace-eip      trace every EIP value to a file TRACE.SSP.  This
                          gets big *fast*.
     -v, --verbose        output verbose messages about debug events.
     -V, --version        output version information and exit
    Example: ssp 0x401000 0x403000 hello.exe

DESCRIPTION

The SSP is a program that uses the Win32 debug API to run a program one ASM instruction at a time. It records the location of each instruction used, how many times that instruction is used, and all function calls. The results are saved in a format that is usable by the profiling program gprof, although gprof will claim the values are seconds, they really are instruction counts. More on that later.

(See also profiler, another profiler that operates in a different fashion: IP sampling. This can provide a different view on your program's operation.)

Because the SSP was originally designed to profile the Cygwin DLL, it does not automatically select a block of code to report statistics on. You must specify the range of memory addresses to keep track of manually, but it's not hard to figure out what to specify. Use the "objdump" program to determine the bounds of the target's ".text" section. Let's say we're profiling cygwin1.dll. Make sure you've built it with debug symbols (else gprof won't run) and run objdump like this:

    $ objdump -h cygwin1.dll

It will print a report like this:

    cygwin1.dll:     file format pei-i386
    Sections:
    Idx Name          Size      VMA       LMA       File off  Algn
      0 .text         0007ea00  61001000  61001000  00000400  2**2
                      CONTENTS, ALLOC, LOAD, READONLY, CODE, DATA
      1 .data         00008000  61080000  61080000  0007ee00  2**2
                      CONTENTS, ALLOC, LOAD, DATA
      . . .

The only information we're concerned with are the VMA of the .text section and the VMA of the section after it (sections are usually contiguous; you can also add the Size to the VMA to get the end address). In this case, the VMA is 0x61001000 and the ending address is either 0x61080000 (start of .data method) or 0x0x6107fa00 (VMA+Size method).

There are two basic ways to use SSP - either profiling a whole program, or selectively profiling parts of the program.

To profile a whole program, just run ssp without options. By default, it will step the whole program. Here's a simple example, using the numbers above:

    $ ssp 0x61001000 0x61080000 hello.exe

This will step the whole program. It will take at least 8 minutes on a PII/300 (yes, really). When it's done, it will create a file called "gmon.out". You can turn this data file into a readable report with gprof:

    $ gprof -b cygwin1.dll

The "-b" means 'skip the help pages'. You can omit this until you're familiar with the report layout. The gprof documentation explains a lot about this report, but ssp changes a few things. For example, the first part of the report reports the amount of time spent in each function, like this:

    Each sample counts as 0.01 seconds.
      %   cumulative   self              self     total
     time   seconds   seconds    calls  ms/call  ms/call  name
     10.02    231.22    72.43       46  1574.57  1574.57  strcspn
      7.95    288.70    57.48      130   442.15   442.15  strncasematch

The "seconds" columns are really CPU opcodes, 1/100 second per opcode. So, "231.22" above means 23,122 opcodes. The ms/call values are 10x too big; 1574.57 means 157.457 opcodes per call. Similar adjustments need to be made for the "self" and "children" columns in the second part of the report.

OK, so now we've got a huge report that took a long time to generate, and we've identified a spot we want to work on optimizing. Let's say it's the time() function. We can use SSP to selectively profile this function by using OutputDebugString() to control SSP from within the program. Here's a sample program:

    	#include <windows.h>
    	main()
    	{
    	  time_t t;
    	  OutputDebugString("ssp on");
    	  time(&t);
    	  OutputDebugString("ssp off");
    	}

Then, add the -d option to ssp to default to *disabling* profiling. The program will run at full speed until the first OutputDebugString, then step until the second. You can then use gprof (as usual) to see the performance profile for just that portion of the program's execution.

There are many options to ssp. Since step-profiling makes your program run about 1,000 times slower than normal, it's best to understand all the options so that you can narrow down the parts of your program you need to single-step.

-v - verbose. This prints messages about threads starting and stopping, OutputDebugString calls, DLLs loading, etc.

-t and -c - tracing. With -t, *every* step's address is written to the file "trace.ssp". This can be used to help debug functions, since it can trace multiple threads. Clever use of scripts can match addresses with disassembled opcodes if needed. Warning: creates *huge* files, very quickly. -c prints each address to the console, useful for debugging key chunks of assembler. Use addr2line -C -f -s -e foo.exe < trace.ssp > lines.ssp and then perl cvttrace to convert to symbolic traces.

-s - subthreads. Usually, you only need to trace the main thread, but sometimes you need to trace all threads, so this enables that. It's also needed when you want to profile a function that only a subthread calls. However, using OutputDebugString automatically enables profiling on the thread that called it, not the main thread.

-l - dll profiling. Generates a pretty table of how much time was spent in each dll the program used. No sense optimizing a function in your program if most of the time is spent in the DLL. I usually use the -v, -s, and -l options:

    $ ssp -v -s -l -d 0x61001000 0x61080000 hello.exe

AUTHOR

DJ Delorie
    Original Author

COPYRIGHT